Station: Lagerschuppen | Short: BHG
Type: Anst | Scale: 1:120 | Module ID: HeMuf390
| Effective length | Effective length (axles) | Remarks
Main tracks
Track Hauptgleis | 750 mm | 14 |
Side tracks
Track 1 | 500 mm | 10 | G-Wagen sind am Schuppen genau zu positionieren da keine Laderampe am Schuppen vorhanden ist
Note: Calculation of effective length based on assumptions: 10 cm effective length correspond to 2 axles.
Loading place | Track | Length | Length (axles) | Remarks to cargo traffic:
Lagerschuppen | 1 | 350 mm | 6
Rampe | 1 | 100 mm | 2
Sum: | 8 |
Distributor/Receiver | Distribution/Receiving | Goods | Car type | Loading place | Car quantity
BHG | R | Düngemittel | G, H, T | Lagerschuppen | 3 / week
R | Futtermittel | G, H, T | Lagerschuppen | 3 / week
R | Zement, gesackt | G, H | Lagerschuppen | 1 / week
R | Baustoffe (Steine, Holz) | G, H, K, R, E, S | Rampe | 2 / week
D | Rüben (Saison) | E | Rampe | 0 / week
D | Getreide (Saison) | T, E, G | Rampe | 0 / week
D | Zuckerrüben (Saison) | E | Rampe | 0 / week
Maschinenausleihstation (MAS) | R | landwirtschaftliches Gerät | G, H, K, R, E, S | Rampe | 1 / week
| Cargo cars quantity |  | General cargo cars quantity |  | Express goods cars quantity
per day | per week | per day | per week | per day | per week
Receiving | 1.4 | 10 | 0 | 0 | 0 | 0
Distribution | 0 | 0 | 0 | 0 | 0 | 0
Total | 1.4 | 10 | 0 | 0 | 0 | 0
Note: The results for the cargo cars quantity are calculated based on assumptions: 7 days a week and no reloading of empty cars!
General remarks to station: Grundstellung "GERADE" der Weiche ist nach Abschluß der Rangierarbeiten dem zuständigen FDL zu melden