Station: Stückgutumschlag | Short: SUM
Type: Anst | Scale: 1:120 | Module ID: EmOtt396
| Effective length | Effective length (axles) | Remarks
Main tracks
Track I-Bahn-Stammgleis | 1800 mm | 36 |
Side tracks
Track 11 | 1000 mm | 20 | Umladung Feuergut
Track 1 | 1500 mm | 30 | Umladung Stückgut
Track 2 | 1500 mm | 30 | Umladung Stückgut
Track 3 | 2000 mm | 40 | Umladung Stückgut
Track 4 | 2000 mm | 40 | Abstellung Wagen
Track 31 | 1800 mm | 36 | Abstellung Wagen / Umfahrung
Note: Calculation of effective length based on assumptions: 10 cm effective length correspond to 2 axles.
Loading place | Track | Length | Length (axles) | Remarks to cargo traffic:
Feuergutrampe | 11 | 1000 mm | 20
Stückgutrampe A | 1 | 1400 mm | 28
Stückgutrampe B | 2 | 1500 mm | 30
Stückgutrampe C | 3 | 1600 mm | 32
Sum: | 110 |
Distributor/Receiver | Distribution/Receiving | Goods | Car type | Loading place | Car quantity
Stückgutumschlag |
| Cargo cars quantity |  | General cargo cars quantity |  | Express goods cars quantity
per day | per week | per day | per week | per day | per week
Receiving | 0 | 0 | 0 | 0 | 0 | 0
Distribution | 0 | 0 | 0 | 0 | 0 | 0
Total | 0 | 0 | 0 | 0 | 0 | 0
Note: The results for the cargo cars quantity are calculated based on assumptions: 7 days a week and no reloading of empty cars!