Station: Irun | Short: IRN
Type: Sbf | Scale: 1:120 | Module ID: GuBue113
| Effective length | Effective length (axles) | Remarks
Main tracks
Track 1 | 3800 mm | 76 | 1.100 bis 3.800 mm - rot
Track 2 | 3800 mm | 76 | 1.100 bis 3.800 mm - blau
Track 3 | 3800 mm | 76 | 1.100 bis 3.800 mm - grün
Track 4 | 3800 mm | 76 | 1.100 bis 3.800 mm - weiß
Track 5 | 3800 mm | 76 | 1.100 bis 3.800 mm - gelb
Track 6 | 3800 mm | 76 | 1.100 bis 3.800 mm - orange
Track 7 | 3800 mm | 76 | 1.100 bis 3.800 mm - schwarz
Track 11 | 220 mm | 4 | Abstellgleis - rot
Track 12 | 220 mm | 4 | Abstellgleis - schwarz
Side tracks
Track 1A | 300 mm | 6 | Abstellgleis - rot
Track 2A | 300 mm | 6 | Abstellgleis - blau
Track 3A | 300 mm | 6 | Abstellgleis - grün
Track 4A | 300 mm | 6 | Abstellgleis - weiß
Track 5A | 300 mm | 6 | Abstellgleis - gelb
Track 6A | 300 mm | 6 | Abstellgleis - orange
Track 7A | 300 mm | 6 | Abstellgleis - schwarz
Note: Calculation of effective length based on assumptions: 10 cm effective length correspond to 2 axles.
| Cargo cars quantity |  | General cargo cars quantity |  | Express goods cars quantity
per day | per week | per day | per week | per day | per week
Receiving | 0 | 0 | 0 | 0 | 0 | 0
Distribution | 0 | 0 | 0 | 0 | 0 | 0
Total | 0 | 0 | 0 | 0 | 0 | 0
Note: The results for the cargo cars quantity are calculated based on assumptions: 7 days a week and no reloading of empty cars!
General remarks to station: Fiddleyard mit Schleppweiche und drehbarer Schiebebühne für TT und H0, bestehend aus max 6 Segmenten a 900 mm. Alle Gleise sind Dreischienengleis für TT und H0. Es können 3, 4, 5 oder 6 Segmente aufgebaut werden, dementsprechend beträgt die nutzbare Gleislänge an Gl. 1 bis 7 jeweils 1.100 mm plus 1x, 2x oder 3x 900 mm bis maximal 3.800 mm, an Gl. 11 und 12 jeweils 220mm, sowie an Gleis 1A bis 7A jeweils 300 mm