Station: Anschluss Werkzeug Maschinen Bau | Short: WMB
Type: Anst | Scale: 1:120 | Module ID: TiSpr384
| Effective length | Effective length (axles) | Remarks
Main tracks
Track Streckengleis | 600 mm | 12 |
Side tracks
Track 2 | 300 mm | 6 |
Note: Calculation of effective length based on assumptions: 10 cm effective length correspond to 2 axles.
Loading place | Track | Length | Length (axles) | Remarks to cargo traffic:
Werkzeugmaschinenbau | 2 | 100 mm | 2
Werkzeugmaschinenbau Kran | 2 | 100 mm | 2
Sum: | 4 |
Distributor/Receiver | Distribution/Receiving | Goods | Car type | Loading place | Car quantity
Werkzeugmaschinenbau | R | Halbzeug | G | Werkzeugmaschinenbau | 1 / week
D | Maschinen in Kiste | R | Werkzeugmaschinenbau Kran | 0.5 / week
D | Werkzeugmaschinen | G | Werkzeugmaschinenbau | 0.5 / week
| Cargo cars quantity |  | General cargo cars quantity |  | Express goods cars quantity
per day | per week | per day | per week | per day | per week
Receiving | 0.1 | 1 | 0 | 0 | 0 | 0
Distribution | 0.1 | 1 | 0 | 0 | 0 | 0
Total | 0.3 | 2 | 0 | 0 | 0 | 0
Note: The results for the cargo cars quantity are calculated based on assumptions: 7 days a week and no reloading of empty cars!