Station: SERO | Short: SERO
Type: Anst | Scale: 1:120 | Module ID: MaRue369
| Effective length | Effective length (axles) | Remarks
Main tracks
Track 1 | 590 mm | 10 |
Note: Calculation of effective length based on assumptions: 10 cm effective length correspond to 2 axles.
Loading place | Track | Length | Length (axles) | Remarks to cargo traffic:
SERO | 1 | 350 mm | 6
Sum: | 6 |
Distributor/Receiver | Distribution/Receiving | Goods | Car type | Loading place | Car quantity
SERO | D | Flaschen, Gläser, Altpapier | G | SERO | 0.5 / day
D | Schrott | E | SERO | 1 / week
D | Glasbruch | E | SERO | 2 / week
| Cargo cars quantity |  | General cargo cars quantity |  | Express goods cars quantity
per day | per week | per day | per week | per day | per week
Receiving | 0 | 0 | 0 | 0 | 0 | 0
Distribution | 0.9 | 6.5 | 0 | 0 | 0 | 0
Total | 0.9 | 6.5 | 0 | 0 | 0 | 0
Note: The results for the cargo cars quantity are calculated based on assumptions: 7 days a week and no reloading of empty cars!