Station: Kranbahn | Short: KRN
Type: Anst | Scale: 1:120 | Module ID: DiThe380
| Effective length | Effective length (axles) | Remarks
Main tracks
Track 1 | 70 cm | 14 |
Track 2 | 135 cm | 26 |
Side tracks
Track 3 | 65 cm | 12 |
Track 4 | 20 cm | 4 |
Track 5 | 82 cm | 16 |
Track 2a | 30 cm | 6 |
Track 2b | 20 cm | 4 |
Track 1b | 34 cm | 6 |
Track 3b | 50 cm | 10 |
Note: Calculation of effective length based on assumptions: 10 cm effective length correspond to 2 axles.
Loading place | Track | Length | Length (axles) | Remarks to cargo traffic:
Ladestraße 1 | 2 | 60 cm | 12
Silo Raiffeisen | 2 | 26 cm | 4
Seitenrampe | 2 | 28 cm | 4
Kopframpe | 2a | 30 cm | 6
Ladestraße 2 | 5 | 82 cm | 16
Ladeplatz | 2 | 60 cm | 12
Ladeplatz | 1 | 60 cm | 12
Sum: | 66 |
Distributor/Receiver | Distribution/Receiving | Goods | Car type | Loading place | Car quantity
Marmorhandel | R | Marmor | G, H | Seitenrampe | / week
D | Marmor | G, H | Seitenrampe | / week
D | Granit | S, R | Ladeplatz | / week
D | Betonteile | S, R, K | Ladeplatz | / week
Baustoffhandel/Raiffeisen | R | Steine | E | Ladestraße 1 | / week
R | Kiese | E, F | Silo Raiffeisen | / week
R | Sand | S, E | Silo Raiffeisen | / week
R | Schnittholz | E, K, R | Ladestraße 1 | / week
Rohrbau | D | Rohre | K, R | Ladestraße 2 | / week
Anlagenbau | R | Stahlteile | K, R, E | Ladeplatz | / week
D | fertige Anlagen | K, R, S | Kopframpe | / week
| Cargo cars quantity |  | General cargo cars quantity |  | Express goods cars quantity
per day | per week | per day | per week | per day | per week
Receiving | NaN | NaN | 0 | 0 | 0 | 0
Distribution | NaN | NaN | 0 | 0 | 0 | 0
Total | NaN | NaN | 0 | 0 | 0 | 0
Note: The results for the cargo cars quantity are calculated based on assumptions: 7 days a week and no reloading of empty cars!
General remarks to station: Die erforderlichen Wagenmengen müssen noch ermittelt werden!