Station: Žst. Výpravčice | Short: XCS Pool
Type: Sbf | Scale: 1:120 | Module ID: PSte042
| Effective length | Effective length (axles) | Remarks
Main tracks
Track | cm | NaN |
Note: Calculation of effective length based on assumptions: 10 cm effective length correspond to 2 axles.
Loading place | Track | Length | Length (axles) | Remarks to cargo traffic:
Güterschuppen |  | cm | NaN
Sum: | NaN |
Distributor/Receiver | Distribution/Receiving | Goods | Car type | Loading place | Car quantity
Glaswerk Svor | D | Quarzglas | G | Güterschuppen | / week
D | Signalglas | G | Güterschuppen | / week
D | Schweissglas | G | Güterschuppen | / week
Möbelindustrie Svor | D | Möbel | G | Güterschuppen | / week
| Cargo cars quantity |  | General cargo cars quantity |  | Express goods cars quantity
per day | per week | per day | per week | per day | per week
Receiving | 0 | 0 | 0 | 0 | 0 | 0
Distribution | NaN | NaN | 0 | 0 | 0 | 0
Total | NaN | NaN | 0 | 0 | 0 | 0
Note: The results for the cargo cars quantity are calculated based on assumptions: 7 days a week and no reloading of empty cars!
General remarks to station: Die allgemeinen Bemerkungen insbesondere die Rangierhinweise müssen noch konkret übersetzt werden!