Station: Hartmannsdorf Großtanklager | Short: HMDTL
Type: Awanst | Scale: 1:120 | Module ID: MaPre237
| Effective length | Effective length (axles) | Remarks
Main tracks
Track Anschluss 1 | mm | NaN |
Track Anschluss 2 | mm | NaN |
Side tracks
Track B | 120 cm | 24 |
Track C | 80 cm | 16 |
Track D | 80 cm | 16 |
Track E | 80 cm | 16 |
Track F | 120 cm | 24 |
Track G | 245 cm | 48 |
Track H | 245 cm | 48 |
Track I | 220 cm | 44 |
Track J | 220 cm | 44 |
Note: Calculation of effective length based on assumptions: 10 cm effective length correspond to 2 axles.
Loading place | Track | Length | Length (axles) | Remarks to cargo traffic: die Gag's müssen Paarisch sein, einem Produktwechsel steht jedoch nichts im Wege Rangierhinweise: - Übernahme, Behandlung und Bereitstellung zur Abfahrt eines Gag's vom Bahnhof innerhalb von 4h. - Max 6 Gag's pro 24h Fahrplan möglich.
Ladegleis 1 | B | 60 cm | 12
Ladegleis 2 | C | 40 cm | 8
Ladegleis 3 | D | 40 cm | 8
Ladegleis 4 | E | 40 cm | 8
Seitenrampe | F | 40 cm | 8
Abstellgruppe | G, H, I, J | 220 cm | 44
Sum: | 88 |
Distributor/Receiver | Distribution/Receiving | Goods | Car type | Loading place | Car quantity
Großtanklager | R | Heizöl | Z | Abstellgruppe | max 5 Gag / day
R | Diesel | Z | Abstellgruppe | max 2 Gag / day
R | Benzin | Z | Abstellgruppe | max 1 Gag / day
D | Heizöl | Z | Abstellgruppe | Wie Empfang / day
D | Diesel | Z | Abstellgruppe | Wie Empfang / day
D | Benzin | Z | Abstellgruppe | Wie Empfang / day
| Cargo cars quantity |  | General cargo cars quantity |  | Express goods cars quantity
per day | per week | per day | per week | per day | per week
Receiving | NaN | NaN | 0 | 0 | 0 | 0
Distribution | NaN | NaN | 0 | 0 | 0 | 0
Total | NaN | NaN | 0 | 0 | 0 | 0
Note: The results for the cargo cars quantity are calculated based on assumptions: 7 days a week and no reloading of empty cars!
General remarks to station: Nur in Verbindung mit Hartmannsdorf!