Station: Bad Baumburg | Short: BBG
Type: Bf | Scale: 1:120 | Module ID: OlBau224
| Effective length | Effective length (axles) | Remarks
Main tracks
Track 1 | 1760 mm | 34 | Hausbahnsteig 680mm
Track 2 | 1550 mm | 30 |
Side tracks
Track 3 | 1550 mm | 30 | Ladestrassengleis
Track 4 | 280 mm | 4 | Verkehrsgleis
Track 4a | 360 mm | 6 |
Track 4b | 390 mm | 6 |
Track 5 | 500 mm | 10 |
Note: Calculation of effective length based on assumptions: 10 cm effective length correspond to 2 axles.
| Track | Length | Remarks to passenger traffic: Kreuzen zweier Personenzüge ist nicht möglich
Platform Hausbahnsteig | 1 | 680 mm
Loading place | Track | Length | Length (axles) | Remarks to cargo traffic:
Güterabfertigung | 4a | 145 mm | 2
Ladestrasse | 3 | 1070 mm | 20
Seitenrampe | 4b | 70 mm | 0
Kopframpe | 5 | 0 mm | 0
Ladestrasse mit Bockkran | 5 | 280 mm | 4
Sum: | 26 |
Distributor/Receiver | Distribution/Receiving | Goods | Car type | Loading place | Car quantity
Kohlen Junker | R | Kohle | E | Ladestrasse | 3 / week
Holz Hansen | D | Stammholz | S, L, R | Ladestrasse | 3 / week
Güterabfertigung | R | Stückgut | G, H | Güterabfertigung | 5 / week
D | Stückgut | G, H | Güterabfertigung | 5 / week
| Cargo cars quantity |  | General cargo cars quantity |  | Express goods cars quantity
per day | per week | per day | per week | per day | per week
Receiving | 1.1 | 8 | 0 | 0 | 0 | 0
Distribution | 1.1 | 8 | 0 | 0 | 0 | 0
Total | 2.3 | 16 | 0 | 0 | 0 | 0
Note: The results for the cargo cars quantity are calculated based on assumptions: 7 days a week and no reloading of empty cars!