Station: Cunnersdorf | Short: CUN
Type: Hp | Scale: 1:120 | Module ID: AnMul316
| Effective length | Effective length (axles) | Remarks
Main tracks
Track Streckengleis | 1961 mm | 38 |
Note: Calculation of effective length based on assumptions: 10 cm effective length correspond to 2 axles.
| Track | Length | Remarks to passenger traffic:
Platform | Streckengleis | 1300 mm
| Cargo cars quantity |  | General cargo cars quantity |  | Express goods cars quantity
per day | per week | per day | per week | per day | per week
Receiving | 0 | 0 | 0 | 0 | 0 | 0
Distribution | 0 | 0 | 0 | 0 | 0 | 0
Total | 0 | 0 | 0 | 0 | 0 | 0
Note: The results for the cargo cars quantity are calculated based on assumptions: 7 days a week and no reloading of empty cars!
General remarks to station: Der Haltepunkt Cunnersdorf (b. Freital) ist nach dem Vorbild an der ehem. Hänichener Kohlenbahn (Windbergbahn) erbaut. Er liegt räumlich neben dem Anschluss Marienschacht und besitzt vorbildentsprechend einen 130 cm langen Bahnsteig am Streckengleis. Zusätzlich sind auf dem Modul 2 Wattenscheider Signalschächte verbaut. Bitte das Modul nur mit Fahrzeugen mit NEM-gerechten Radsätzen befahren!