Station: Beli Breg - Бели Брег | Short: XBEB
Type: Bf | Scale: 1:120.0 | Module ID: EmCha602 (CMRBu_2210)
| Effective length | Effective length (axles) | Remarks
Main tracks
Track 1 | 1550.0 mm | 30 |
Side tracks
Track 2 | 1400.0 mm | 28 |
Note: Calculation of effective length based on assumptions: 10 cm effective length correspond to 2 axles.
| Track | Length | Remarks to passenger traffic:
Platform | 1 | 500.0 mm
Loading place | Track | Length | Length (axles) | Remarks to cargo traffic:
Rampe | 2 | 1200.0 mm | 24
Sum: | 24 |
Distributor/Receiver | Distribution/Receiving | Goods | Car type | Loading place | Car quantity
Mine | R | Leer für Kohle | E | Rampe | 24.0 / day
D | Kohle | E | Rampe | 24.0 / day
| Cargo cars quantity |  | General cargo cars quantity |  | Express goods cars quantity
per day | per week | per day | per week | per day | per week
Receiving | 24 | 168 | 0 | 0 | 0 | 0
Distribution | 24 | 168 | 0 | 0 | 0 | 0
Total | 48 | 336 | 0 | 0 | 0 | 0
Note: The results for the cargo cars quantity are calculated based on assumptions: 7 days a week and no reloading of empty cars!