Station: Vitezny Unor | Short: XCS Pool
Type: Anst | Scale: 1:120 | Module ID:
| Effective length | Effective length (axles) | Remarks
Main tracks
Track | cm | NaN |
Note: Calculation of effective length based on assumptions: 10 cm effective length correspond to 2 axles.
Loading place | Track | Length | Length (axles) | Remarks to cargo traffic:
Ladefläche |  | cm | NaN
Sum: | NaN |
Distributor/Receiver | Distribution/Receiving | Goods | Car type | Loading place | Car quantity
Sägewerk "Vitezny Unor" | R | Stammholz | R, E | Ladefläche | / week
D | Bretter | R | Ladefläche | / week
D | Latten | R | Ladefläche | / week
D | Balken | R | Ladefläche | / week
| Cargo cars quantity |  | General cargo cars quantity |  | Express goods cars quantity
per day | per week | per day | per week | per day | per week
Receiving | NaN | NaN | 0 | 0 | 0 | 0
Distribution | NaN | NaN | 0 | 0 | 0 | 0
Total | NaN | NaN | 0 | 0 | 0 | 0
Note: The results for the cargo cars quantity are calculated based on assumptions: 7 days a week and no reloading of empty cars!