Station: Görzig | Short: GZG
Type: Hst | Scale: 1:120 | Module ID: HaPeiXXX
| Effective length | Effective length (axles) | Remarks
Main tracks
Track 1 | 91.7 cm | 18 | Streckengleis
Side tracks
Track 2 | 70.8 cm | 14 |
Track 2a | 29 cm | 4 |
Note: Calculation of effective length based on assumptions: 10 cm effective length correspond to 2 axles.
| Track | Length | Remarks to passenger traffic:
Platform | 1 | 41.6 cm
Loading place | Track | Length | Length (axles) | Remarks to cargo traffic:
Ladestraße | 2, 2a | 75 cm | 14
Rampe | 2 | 12.5 cm | 2
Sum: | 16 |
Distributor/Receiver | Distribution/Receiving | Goods | Car type | Loading place | Car quantity
VEG Görzig West | R | Tierfutter | G, E | Ladestraße | / week
D | landwirtschlaftliche Produkte (Getreide, Kartoffel, Mais, Milch) | G, H, E | Rampe, Ladestraße | / week
Kohlenhandel Russwurm Görzig | R | Kohle | E | Ladestraße | / week
Baustoffhandel Baumann Rietz-Neuendorf | R | Baustoffe | G, H | Rampe | / week
| Cargo cars quantity |  | General cargo cars quantity |  | Express goods cars quantity
per day | per week | per day | per week | per day | per week
Receiving | NaN | NaN | 0 | 0 | 0 | 0
Distribution | NaN | NaN | 0 | 0 | 0 | 0
Total | NaN | NaN | 0 | 0 | 0 | 0
Note: The results for the cargo cars quantity are calculated based on assumptions: 7 days a week and no reloading of empty cars!