Station: Anschluß Kalkwerk | Short: KW
Type: Anst, Awanst | Scale: 1:120 | Module ID: JoLan364
| Effective length | Effective length (axles) | Remarks
Main tracks
Track 1 | 650 mm | 12 |
Side tracks
Track 10 | 230 mm | 4 | Umschlaggleis
Track 10a | 100 mm | 2 |
Note: Calculation of effective length based on assumptions: 10 cm effective length correspond to 2 axles.
Loading place | Track | Length | Length (axles) | Remarks to cargo traffic:
Umschlaggleis | 1 | 230 mm | 4
Sum: | 4 |
Distributor/Receiver | Distribution/Receiving | Goods | Car type | Loading place | Car quantity
VEB Kalkwerk Ernst Thählmann | R | Leerwagen | K, T, U | Umschlaggleis | 2 / week
D | Kalk | K, T, U | Umschlaggleis | 2 / week
| Cargo cars quantity |  | General cargo cars quantity |  | Express goods cars quantity
per day | per week | per day | per week | per day | per week
Receiving | 0.3 | 2 | 0 | 0 | 0 | 0
Distribution | 0.3 | 2 | 0 | 0 | 0 | 0
Total | 0.6 | 4 | 0 | 0 | 0 | 0
Note: The results for the cargo cars quantity are calculated based on assumptions: 7 days a week and no reloading of empty cars!