Station: VEB Kohlehandel | Short: KHL
Type: Anst | Scale: 1:120 | Module ID: LuRau375
| Effective length | Effective length (axles) | Remarks
Main tracks
Track I-Bahn-Stammgleis | 200 cm | 40 |
Side tracks
Track 1 | 90 cm | 18 | Entladung E-Wagen
Track 2a | 100 cm | 20 | Entladung F-Wagen
Track 2b | 40 cm | 8 | Entladung Flüssiggas
Note: Calculation of effective length based on assumptions: 10 cm effective length correspond to 2 axles.
Loading place | Track | Length | Length (axles) | Remarks to cargo traffic:
Entladung Flüssiggas | 2b | 40 cm | 8
Entladung E-Wagen | 1 | 90 cm | 18
Entladung F-Wagen | 2a | 100 cm | 20
Sum: | 46 |
Distributor/Receiver | Distribution/Receiving | Goods | Car type | Loading place | Car quantity
VEB Kohlehandel | R | Flüssiggas | G U Z | Entladung Flüssiggas | 3 / week
R | Flüssiggas in Flaschen | G | Entladung Flüssiggas | 2 / week
R | Leere Flüssiggasflaschen | G | Entladung Flüssiggas | 1 / week
R | Steinkohlenkoks | E Fc | Entladung E-Wagen, Entladung F-Wagen | 10 / week
R | Braunkohlenbriketts | E Fc | Entladung E-Wagen, Entladung F-Wagen | 50 / week
R | Braunkohlengries | E Fc | Entladung E-Wagen, Entladung F-Wagen | 4 / week
R | Fettkohle | E Fc | Entladung E-Wagen, Entladung F-Wagen | 1 / week
R | Petroleum in Gebinden | G | Entladung Flüssiggas | 1 / week
R | Acetylen in Flaschen | G | Entladung Flüssiggas | 0.25 / week
R | Stickstoff in Flaschen | G | Entladung Flüssiggas | 0.25 / week
R | Sauerstoff in Flaschen | G | Entladung Flüssiggas | 0.25 / week
D | Gasflaschen zur Aufarbeitung | G | Entladung Flüssiggas | 0.5 / week
| Cargo cars quantity |  | General cargo cars quantity |  | Express goods cars quantity
per day | per week | per day | per week | per day | per week
Receiving | 10.4 | 72.75 | 0 | 0 | 0 | 0
Distribution | 0.1 | 0.5 | 0 | 0 | 0 | 0
Total | 10.5 | 73.25 | 0 | 0 | 0 | 0
Note: The results for the cargo cars quantity are calculated based on assumptions: 7 days a week and no reloading of empty cars!