Station: Sägewerk MEC | Short: SWMEC
Type: Anst | Scale: 1:120 | Module ID: MaHem360
| Effective length | Effective length (axles) | Remarks
Main tracks
Track 1 | 122 cm | 24 |
Side tracks
Track 2 | 66 cm | 12 |
Track 2a | 36 cm | 6 |
Note: Calculation of effective length based on assumptions: 10 cm effective length correspond to 2 axles.
Loading place | Track | Length | Length (axles) | Remarks to cargo traffic:
Ladestraße | 2 | 66 cm | 12
Ladestraße | 2a | 36 cm | 6
Sum: | 18 |
Distributor/Receiver | Distribution/Receiving | Goods | Car type | Loading place | Car quantity
VEB Astloch | R | Hochholz | E, R | Ladestraße | 8 / day
R | Heizöl | Z | Ladestraße | 1 / week
R | Maschinenteile | G | Ladestraße | 1 / week
D | Hackschnitzel | E | Ladestraße | 2 / day
D | Bretter | R | Ladestraße | 2 / day
D | Paletten | E, G | Ladestraße | 2 / day
| Cargo cars quantity |  | General cargo cars quantity |  | Express goods cars quantity
per day | per week | per day | per week | per day | per week
Receiving | 8.3 | 58 | 0 | 0 | 0 | 0
Distribution | 6 | 42 | 0 | 0 | 0 | 0
Total | 14.3 | 100 | 0 | 0 | 0 | 0
Note: The results for the cargo cars quantity are calculated based on assumptions: 7 days a week and no reloading of empty cars!
General remarks to station: