Station: Bw G-Ost | Short: BGO
Type: Bw | Scale: 1:120 | Module ID: JuGra290
| Effective length | Effective length (axles) | Remarks
Main tracks
Track 5 | 118 cm | 22 | Haupteinfahrgleis
Side tracks
Track 1 | 143 cm | 28 | Achtung: Länge gilt nur bis zur Abzweigweiche des ersten Lokschuppens!
Track 2 | 120 cm | 24 |
Track 3 | 194 cm | 38 |
Track 4 | 124 cm | 24 |
Track 6 | 48 cm | 8 |
Track 7 | 118 cm | 22 |
Track 8 | 138 cm | 26 |
Track 9 | 69 cm | 12 |
Track 10 | 28 cm | 4 |
Track 11 | 62 cm | 12 |
Track 12 | 55 cm | 10 |
Track 13 | 67 cm | 12 |
Track 14 | 56 cm | 10 |
Track 15 | 50 cm | 10 |
Note: Calculation of effective length based on assumptions: 10 cm effective length correspond to 2 axles.
Loading place | Track | Length | Length (axles) | Remarks to cargo traffic:
Materiallager | 10 | cm | NaN
VT-Schuppen | 14, 15 | cm | NaN
Kohlebansen | 6 | cm | NaN
Tankstelle | 11 | cm | NaN
Sum: | NaN |
Distributor/Receiver | Distribution/Receiving | Goods | Car type | Loading place | Car quantity
| Cargo cars quantity |  | General cargo cars quantity |  | Express goods cars quantity
per day | per week | per day | per week | per day | per week
Receiving | 0 | 0 | 0 | 0 | 0 | 0
Distribution | 0 | 0 | 0 | 0 | 0 | 0
Total | 0 | 0 | 0 | 0 | 0 | 0
Note: The results for the cargo cars quantity are calculated based on assumptions: 7 days a week and no reloading of empty cars!