Station: Anschluss Viehrampe | Short: AVR
Type: Anst | Scale: 1:120 | Module ID: HaSan387
| Effective length | Effective length (axles) | Remarks
Main tracks
Track Streckengleis | 900 mm | 18 |
Side tracks
Track 1 | 380 mm | 6 | Laderampe
Note: Calculation of effective length based on assumptions: 10 cm effective length correspond to 2 axles.
Loading place | Track | Length | Length (axles) | Remarks to cargo traffic:
Viehrampe | 1 | 150 mm | 2
Kopf-/ Seitenrampe | 1 | 80 mm | 0
Sum: | 2 |
Distributor/Receiver | Distribution/Receiving | Goods | Car type | Loading place | Car quantity
LPG (T) Kuhfraß | R | Zuchtbullen | G, H | Viehrampe | 0.5 / week
R | Ersatzteile | G, H, K | Kopf-/ Seitenrampe | 0.5 / week
R | Traktor | K, R | Kopf-/ Seitenrampe | 0.25 / week
R | Futterrüben | E | Kopf-/ Seitenrampe | 2 / week
R | Ohrmarkenrohlinge | G, H | Kopf-/ Seitenrampe | 0.25 / week
R | Heu | K | Kopf-/ Seitenrampe | 0.5 / week
R | Mastfutter | G, H, T | Kopf-/ Seitenrampe | 3 / week
D | Färsen | G, H | Viehrampe | 2 / week
D | Zuchtbullen | G, H | Viehrampe | 1 / week
D | Traktor zur Reparatur | K, R | Kopf-/ Seitenrampe | 0.25 / week
D | Schlachtrinder | G, H | Viehrampe | 3 / week
LPG (P) Kuhfraß | R | Traktor, Landmaschine | K, R | Kopf-/ Seitenrampe | 0.25 / week
R | Saatgut | G, H, T | Kopf-/ Seitenrampe | 2 / week
R | Ersatzteile | G, H, K | Kopf-/ Seitenrampe | 0.5 / week
D | Traktor zur Reparatur | K, R | Kopf-/ Seitenrampe | 0.25 / week
D | Saatgut | G, H | Kopf-/ Seitenrampe | 1 / week
| Cargo cars quantity |  | General cargo cars quantity |  | Express goods cars quantity
per day | per week | per day | per week | per day | per week
Receiving | 1.4 | 9.75 | 0 | 0 | 0 | 0
Distribution | 1.1 | 7.5 | 0 | 0 | 0 | 0
Total | 2.5 | 17.25 | 0 | 0 | 0 | 0
Note: The results for the cargo cars quantity are calculated based on assumptions: 7 days a week and no reloading of empty cars!
General remarks to station: Anschlussstelle ist mit Gleissperre gesichert