Station: Erdweg | Short: EWG
Type: Anst | Scale: 1:120 | Module ID: HeMuf391
| Effective length | Effective length (axles) | Remarks
Main tracks
Track Strecke | mm | NaN |
Side tracks
Track 1 | 500 mm | 10 |
Note: Calculation of effective length based on assumptions: 10 cm effective length correspond to 2 axles.
Loading place | Track | Length | Length (axles) | Remarks to cargo traffic:
Hochrampe | 1 | 430 mm | 8
Sum: | 8 |
Distributor/Receiver | Distribution/Receiving | Goods | Car type | Loading place | Car quantity
VEB Bauzuschlagstoffe, Werk IV, Steinbruch Erdweg | D | Schotter | E,F,X | Hochrampe | 4 / day
D | Splitt | E,F | Hochrampe | 3 / day
D | Kies | E, F | Hochrampe | 2 / day
VEG Erdweg | D | Zuckerrüben (Saison) | E | Hochrampe | 0 / day
| Cargo cars quantity |  | General cargo cars quantity |  | Express goods cars quantity
per day | per week | per day | per week | per day | per week
Receiving | 0 | 0 | 0 | 0 | 0 | 0
Distribution | 9 | 63 | 0 | 0 | 0 | 0
Total | 9 | 63 | 0 | 0 | 0 | 0
Note: The results for the cargo cars quantity are calculated based on assumptions: 7 days a week and no reloading of empty cars!
General remarks to station: Die Grundstellung der Weiche "Gerade" ist dem zuständigen FDL nach Ende der Rangierfahrt zu melden